{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Cube wandbündig 12 mm"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":28,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cube wandbündig 12 mm","index":0,"n_rows":42,"n_cols":26,"rows_kept":42,"cut":false,"hidden":false,"merged":[[0,1,0,3],[1,1,1,3],[2,1,2,3]]}
[{"$f":"VLOOKUP(\"Taal\",TabVertalingen,Hulp,FALSE)","v":"Sprache"},"DE",null,null,"q",null,"Type","S/D","Maat","Min B","Max B","A","E","B","H","F","I","C",null,null,"NL","EN","DE",null,"Hulp","HulpRij"]
[{"$f":"VLOOKUP(\"Kozijnsysteem\",TabVertalingen,Hulp,FALSE)","v":"Zargesystem"},"Cube wandbündig 12 mm",null,null,"q",null,null,null,null,"maat B","maat B","Structural wall opening","Subframe outer dimension","Door dimension","Frame rebate dimension","Frame outer dimension","Frame outer edge dimension","Clearance dimension","Ventilation space under door",null,"Cube op de wand","Cube on the wall with","Wandumfassend mit ausstemmen",null,{"$f":"MATCH(Taal,Talen,0)","v":3},{"$f":"MATCH(Soort,OFFSET(Soorten,,Hulp-1),0)","v":6}]
[{"$f":"VLOOKUP(\"Enkeldeur/ dubbeldeur\",TabVertalingen,Hulp,FALSE)","v":"1-flügelig/ 2-flügelig"},"1-flügelig",null,null,"q",null,"Cube op de wand","Single","Breedte",500,1235,51,null,0,7,111,32,-19,null,null,"Cube op de wand zonder uitkap","Cube on the wall without","Wandumfassend ohne ausstemmen"]
[null,null,null,null,null,null,"Cube op de wand","Single","Hoogte",1800,3000,38,null,0,8,60,20,-5,5,null,"RE-Cube op de wand","RE-Cube on the wall","Wandumfassend Reverse"]
[null," ",{"$f":"VLOOKUP(\"Breedte\",TabVertalingen,Hulp,FALSE)","v":"Breite"},{"$f":"VLOOKUP(\"Hoogte\",TabVertalingen,Hulp,FALSE)","v":"Höhe "},null,null,"Cube op de wand","Double","Breedte",1000,2400,68,null,0,7,111,32,-19,null,null,"Cube flush 6 mm","Cube  flush 6 mm","Cube wandbündig 6 mm"]
[{"$f":"VLOOKUP(\"Ruwbouw sparingmaat\",TabVertalingen,Hulp,FALSE)","v":"Maueröffnungsmaße"},"A",null,null,null,null,"Cube op de wand","Double","Hoogte",1800,3000,38,null,0,8,60,20,-5,5,null,"RE-Cube flush 6 mm","RE-Cube flush 6 mm","RE-Cube wandbündig 6 mm"]
[{"$f":"VLOOKUP(\"Stelkozijn buitenmaat\",TabVertalingen,Hulp,FALSE)","v":"Blindstockaußenmaße"},"E",null,null,null,null,"Cube op de wand zonder uitkap","Single","Breedte",500,1235,76,null,0,7,111,32,-19,null,null,"Cube flush 12 mm","Cube flush 12 mm","Cube wandbündig 12 mm"]
[{"$f":"VLOOKUP(\"Deurblad\",TabVertalingen,Hulp,FALSE)","v":"Türblattaussenmaß"},"B",null,null,null,null,"Cube op de wand zonder uitkap","Single","Hoogte",1800,3000,38,null,0,8,60,20,-5,5,null,"RE-Cube flush 12 mm","RE-Cube flush 12 mm","RE-Cube wandbündig 12 mm"]
[{"$f":"VLOOKUP(\"Kozijn opdekmaat\",TabVertalingen,Hulp,FALSE)","v":"Zargenfalzmaße"},"H",null,null,null,null,"Cube op de wand zonder uitkap","Double","Breedte",1000,2400,91,null,0,7,111,32,-19,null,null,"Cube SF","Cube SF","Cube SF"]
[{"$f":"VLOOKUP(\"Kozijn buitenmaat\",TabVertalingen,Hulp,FALSE)","v":"Bekleidungs-außenmaße"},"F",null,null,null,null,"Cube op de wand zonder uitkap","Double","Hoogte",1800,3000,38,null,0,8,60,20,-5,5,null,"Undercover","Undercover","Undercover"]
[{"$f":"VLOOKUP(\"Kozijn binnenmaat\",TabVertalingen,Hulp,FALSE)","v":"Futteraußenmaße"},"I",null,null,null,null,"RE-Cube op de wand","Single","Breedte",500,1235,76,null,0,7,111,66,-19,null,null,"RE-Undercover","RE-Undercover","RE-Undercover"]
[{"$f":"VLOOKUP(\"Vrije doorgang\",TabVertalingen,Hulp,FALSE)","v":"Durchgangsmaße"},"C",null,null,null,null,"RE-Cube op de wand","Single","Hoogte",1800,3000,43,null,0,8,60,34,-5,5,null,"Ruwbouw sparingmaat","Structural wall opening","Maueröffnungsmaße"]
[{"$f":"VLOOKUP(\"Ruimte onder de deur\",TabVertalingen,Hulp,FALSE)","v":"Bodenluft"},null,null,5,null,null,"RE-Cube op de wand","Double","Breedte",1000,2400,76,null,0,7,111,66,-19,null,null,"Stelkozijn buitenmaat","Subframe outer dimension","Blindstockaußenmaße"]
[null,null,null,null,null,null,"RE-Cube op de wand","Double","Hoogte",1800,3000,43,null,0,8,60,34,-5,5,null,"Deurblad","Door dimension","Türblattaussenmaß"]
[null,null,null,null,null,null,"Cube flush 6 mm","Single","Breedte",500,1235,147,127,0,7,111,32,-19,null,null,"Kozijn opdekmaat","Frame rebate dimension","Zargenfalzmaße"]
[null,null,null,null,null,null,"Cube flush 6 mm","Single","Hoogte",1800,3000,78,68,0,8,60,20,-5,5,null,"Kozijn buitenmaat","Frame outer dimension","Bekleidungs-außenmaße"]
[null,null,null,null,null,null,"Cube flush 6 mm","Double","Breedte",1000,2400,147,127,0,7,111,32,-19,null,null,"Kozijn binnenmaat","Frame outer edge dimension","Futteraußenmaße"]
["Alle Maßen in mm",null,null,null,null,null,"Cube flush 6 mm","Double","Hoogte",1800,3000,78,68,0,8,60,20,-5,5,null,"Vrije doorgang","Clearance dimension","Durchgangsmaße"]
[null,null,null,null,null,null,"RE-Cube flush 6 mm","Single","Breedte",500,1235,147,127,0,7,111,66,-19,null,null,"Ruimte onder de deur","Ventilation space under door","Bodenluft"]
[null,null,null,null,null,null,"RE-Cube flush 6 mm","Single","Hoogte",1800,3000,78,68,0,8,60,34,-5,5,null,"Breedte","Width","Breite"]
[null,null,null,null,null,null,"RE-Cube flush 6 mm","Double","Breedte",1000,2400,147,127,0,7,111,66,-19,null,null,"Hoogte","Height","Höhe "]
[null,null,null,null,null,null,"RE-Cube flush 6 mm","Double","Hoogte",1800,3000,78,68,0,8,60,34,-5,5,null,"Enkel","Single","1-flügelig"]
[null,null,null,null,null,null,"Cube flush 12 mm","Single","Breedte",500,1235,161,139,0,7,111,32,-19,null,null,"Dubbel","Double","2-flügelig"]
[null,null,null,null,null,null,"Cube flush 12 mm","Single","Hoogte",1800,3000,84,74,0,8,60,20,-5,5,null,"Taal","Language","Sprache"]
[null,null,null,null,null,null,"Cube flush 12 mm","Double","Breedte",1000,2400,161,139,0,7,111,32,-19,null,null,"Kozijnsysteem","Framesystem","Zargesystem"]
[null,null,null,null,null,null,"Cube flush 12 mm","Double","Hoogte",1800,3000,84,74,0,8,60,20,-5,5,null,"Enkeldeur/ dubbeldeur","Single/ double","1-flügelig/ 2-flügelig"]
[null,null,null,null,null,null,"RE-Cube flush 12 mm","Single","Breedte",500,1235,161,139,0,7,111,66,-19]
[null,null,null,null,null,null,"RE-Cube flush 12 mm","Single","Hoogte",1800,3000,83,74,0,8,60,34,-5,5]
[null,null,null,null,null,null,"RE-Cube flush 12 mm","Double","Breedte",1000,2400,161,139,0,7,111,66,-19]
[null,null,null,null,null,null,"RE-Cube flush 12 mm","Double","Hoogte",1800,3000,83,74,0,8,60,34,-5,5]
[null,null,null,null,null,null,"Cube SF","Single","Breedte",500,1235,87,78,0,7,73,32,-19]
[null,null,null,null,null,null,"Cube SF","Single","Hoogte",1800,3000,53,44,0,8,41,20,-4,5]
[null,null,null,null,null,null,"Cube SF","Double","Breedte",1000,2400,93,78,0,7,73,32,-19]
[null,null,null,null,null,null,"Cube SF","Double","Hoogte",1800,3000,53,44,0,8,41,20,-4,5]
[null,null,null,null,null,null,"Undercover","Single","Breedte",500,1235,76,null,0,7,157,37,-23]
[null,null,null,null,null,null,"Undercover","Single","Hoogte",1800,2950,38,null,0,8,83,23,-7,5]
[null,null,null,null,null,null,"Undercover","Double","Breedte",1000,2400,86,null,0,7,157,37,-23]
[null,null,null,null,null,null,"Undercover","Double","Hoogte",1800,2950,38,null,0,8,83,23,-7,5]
[null,null,null,null,null,null,"RE-Undercover","Single","Breedte",500,1235,76,null,0,7,157,37,-23]
[null,null,null,null,null,null,"RE-Undercover","Single","Hoogte",1800,2950,38,null,0,8,83,23,-7,5]
[null,null,null,null,null,null,"RE-Undercover","Double","Breedte",1000,2400,86,null,0,7,157,37,-23]
[null,null,null,null,null,null,"RE-Undercover","Double","Hoogte",1800,2950,38,null,0,8,83,23,-7,5]